avrdude: stk500v2_ReceiveMessage(): timeout

avrdude: AVR device initialized and ready to accept instructions

Reading | ################################################## | 100% 0.03s

avrdude: Device signature = 0x504943
avrdude: NOTE: "flash" memory has been specified, an erase cycle will be performed
         To disable this feature, specify the -D option.
avrdude: erasing chip
avrdude: reading input file "blinker.hex"
avrdude: ERROR: address 0x1d000100 out of range at line 3 of blinker.hex
avrdude: read from file 'blinker.hex' failed

avrdude: safemode: Fuses OK (H:00, E:00, L:00)

avrdude done.  Thank you.

