MARLIN - open "Marlin.ino" in Arduino. This is the currently uploaded firmware on the device (working)

PrintRun - Contains the Pronterface.exe program to drive printer, and the Slic3r folder with some good, working settings.

PrintRun seems to work best placed on the root directory of C:
